Connect SatLoc Bantam to Reabe Smart Gate.
Rev A
Gate Software A0  08 or Higher
Satloc Software V 5.5.31.5 or Higher 
GPS Paint wires can be connected to Pins 5 and 6 of Open Close Switch.

Wire GPS to Controller:
	Concetion
	Wire Reabe 232 GPS
	 
	Conection
	Wire Satloc
	Plug Pin

	Gnd Reabe
	Shield
	>->
	GND
	GRN or SH
	5

	232 In
	Wht/Blue
	>->
	232 TX
	RED
	3

	232 Out
	White
	>->
	232 RX
	WHT
	2


Cable End if Desired.

 
What lines will he need to tie into to get the Speed data out.
You have a couple choices here. 
1. You can purchase one of our cables, but you’ll likely want to cut off the other end and replace it with a connector of your choosing.  Such a cable can ship today. 
2. You can purchase the CONXALL 3282-8PG-321 and wire it up as below.  The RTS/CTS are not needed.

Here are some links to that connector:
https://www.eciaauthorized.com/en/part/conxall/3282-8PG-321
 
https://www.sager.com/3282-8pg-321-1107420.html
 
https://www.digikey.com/product-detail/en/conxall-switchcraft/3282-8PG-321/SC3158-ND/3514169



Hello David,

I am sending you the GPS connection Data so you have it all in one place.

The software is at:
https://www.reabeair.com/wp-content/uploads/2021/11/AirBantam_5.5.31.5.zip

A hook up guide is at:
https://www.reabeair.com/wp-content/uploads/2021/11/Connect-SatLoc-Bantam-to-Reabe-Smart-Gate-REV-1.docx

I did send the wire info.
Satloc is checking in on the TX and RX lines.

Because a serial Connection goes as shown:
GPS----Gate
TX--->---RX
RX---<---TX

They did not know if the TX Label is for the GPS or the Gate.

On the G4, 
The White line is there RX line that goes to my White TX line
The Red line is there TX line that goes to my Wht/Blue RX line
I would guess it to be the same for the Bantam.
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